Frequently Asked Questions (FAQ)

Many thanks to Mike Fitzhugh for collecting questions and answers from
mailing list and forum!

     1. General Questions
     2. Extraction Questions
     3. Compression Questions
     4. Offset Questions
     5. Write Questions
     6. WAV Editor Questions
     7. Utilities Questions


1. General Questions

 Q:What is EAC?
 A:EAC is "Exact Audio Copy". It will help you to copy (extract) audio
   tracks, or even parts of them, to the harddisk. In newer versions it
   also includes some audio CD writing routines and a small audio editor.


 Q:Why should I use EAC, instead of AudioGrabber, WinDAC, etc.
 A:EAC features some special read modes, known as "Secure Modes". Using
   these secure modes, every sector read will be doublechecked and reread
   or corrected if necessary. On many drives the extraction is not error
   free, thus these routines will make sure the track is read correctly.


 Q:Audio extraction is purely digital, how could unremarked errors occur?
 A:The data transmission itself is purely digital and also the data stored
   on the CD. But the Red Book standard (standard for audio CDs) is very
   weak and only little error correction will be performed in the drive.
   So on bad CD-ROM drives it is possible that you receive erroneous
   results.


 Q:I want to install a newer version of EAC, do I have to uninstall the
   previous install first?
 A:Unless otherwise indicated on a new release, for updates just extract
   the new exe file in your EAC dir. (I.e. overwrite the old exe) and you
   will retain the old settings. If you want to delete the old options
   nevertheless, just delete the key
   HKEY_CURRENT_USER\Software\AWSoftware\EAC .


 Q:Where is the official homepage for EAC? Where can I download new
   versions?
 A:It is at http://www.ExactAudioCopy.de/ There you will find a download
   page and a forum for persons who dislike the mailing list, but is not
   as good supported as the mailing list.


 Q:I downloaded the file EAC.ZIP from your homepage. Whenever I
   doubleclick on the file a text editor opens and shows garbage. How can
   I start EAC?
 A:A ZIP file contains compressed files. This is easier for the
   transmission of several files. For decompression you need an UnZIP
   program like WinZIP.


 Q:I only own a very bad soundcard, or no soundcard at all... Does this
   matters?
 A:No, your soundcard has nothing to do with ripping or burning cds. If
   you use digital extraction (which EAC does), you are not using the
   soundcard to create the wav, it's read directly from the cd.


 Q:What is meant by "on-the-fly" ?
 A:This means that one action is performed while (or intermixed with)
   another action. So e.g. if you extract and compress at once (and not
   extract first and compress afterwards), you could call it on-the-fly
   compression.


 Q:What are gaps (pre-track gaps)?
 A:When playing an audio CD in a standalone player, often the time display
   will show up negative values before actually starting a track. This gap
   is usually used for seperate two different tracks. If jumping to a
   specific track, it will start with the actual music, only when running
   into a track the gap occurs.


 Q:Is it possible to extract audio digitally from a (Video) DVD?
 A:Yes, but not using EAC and though it's more manual work. The only
   hardware you will need is a DVD drive and special software for removing
   the CSS (on commercial DVDs) and demultiplex the VOB files into the
   audio streams (usually compressed in AC3 or DTS). Then you need a
   programm to decompress these compressed files (a AC3 decompressor or a
   DTS decompressor).
   "Real" Audio DVDs are planned, but are not released yet, as the copy
   protection scheme will be improved first.


 Q:Do you plan to release a Linux or MAC version of EAC?
 A:Sorry, no Linux nor MAC version is planned at all. But it is reported
   that EAC runs in an emulation layer (WINE for Linux and Virtual PC Win
   98 for MAC), so if you own this software have a try.


 Q:I use Windows NT/2000, but EAC seems to have problems to store the
   options or get any SCSI response.
 A:Make sure you start EAC from an admin account, as some functions need a
   to access low level system routines, which are not accessable from user
   accounts. If you use the "Native SCSI Interface", try the "ASPI
   Interface" instead, perhaps it will already help.
   A user send this suggestion, feel free to try it out :
   In administrator mode, Start, Run, MMC
   Console Menu, Add/Remove Snap-in
   Add.
   Group Policy
   (Group Policy will be shown as "Local Computer Policy". Go figure :P -
   actually, if your computer receives its policies from a network server,
   it won't show and you'll have to set it directly on the server, ask
   your admin then. )
   Ok
   On the tree, Console Root, Local Computer Policy, Computer
   Configuration, Windows Settings, Security Settings, Local Policies,
   Security Options
   Find "Restrict CD-ROM access to locally logged-on user only". It should
   be disabled by default. Enable it.
   No need to reboot, when quitting MMC, no need to save.
   What this does is allow any local software to lock the drive for
   exclusive use. What this removes is the ability to use the CD-Rom as a
   Terminal Services client. With this, EAC works seamlessly. It also
   makes it possible to use a CD-Writer as restricted user with whatever
   software you choose.


 Q:When trying to install EAC in Windows NT or Windows 2000, I get the
   following error message: "The DLL WNASPI32.DLL could not be found in
   the specified path" then a list of paths. I searched my hard drives and
   the named DLL does not exist on my machine. I found the DLL on the web
   and installed it into windows\system32\. Then I tried to re-install EAC
   and got the following error message: "The ASPI interface could not be
   initialized correctly! (Error E4h) (ASPI for Windows failed init)".
   What now?
 A:EAC needs a driver called "ASPI", it is an SCSI driver, but works also
   with IDE CD-ROM drives (not a single file, but a complete package, so
   installing just the DLL won't help). It is included in Win95/98, but
   not in Windows NT/2000. The newer versions of EAC should not absolute
   need ASPI anymore, but ASPI would be nevertheless the most stable. ASPI
   is available from different manufacturers (of SCSI interface cards),
   but it seems that the only working one with EAC is coming from Adaptec.
   First of all you should upgrade to a newer version of EAC, as ASPI is
   not absolutely necessary any more.


 Q:What is the difference between ASPI, ASAPI and Native drivers?
 A:EAC communicates directly with the CD-ROM drives. For this EAC make use
   of several interfaces which do the low level work. You can choose the
   interface by your own in the EAC options (depending which interfaces
   are installed in your computer).
   ASPI is from Adaptec, it comes preinstalled in Win95/98. In all other
   Windows it needs to be installed, but in these OS the installer tests
   if any Adaptec hardware is in your computer. Nevertheless you can try
   to install it, download here.
   VOB produced a replacement called ASAPI. It is freely available from
   here.
   In WinNT/2000/XP EAC is able to use a native interface in that OS. This
   is still buggy and only recommended when you don't want to install 3rd
   party software. Nevertheless, this will only work if you are logged in
   with admin rights. If you encounter problems, it is strongly
   recommended to download ASAPI and to change the interface to that.


2. Extraction Questions

 Q:In the column "Copy Protection" is always "Yes" denoted. What does it
   mean, will it not be possible to extract the tracks?
 A:It is possible also to extract copy protected tracks, as the copy
   protection is only a flag on the CD, and all CD-ROM drives will ignore
   it on reading. Some month ago there are now also real copy protections
   for audio CDs, but this information is not given in the table. If there
   is such a CD, it will show garbage, not extract tracks or probably
   insert errors in the extraction.


 Q:I extracted all tracks of an audio CD and tried to write them back to
   CD, but the writing application tells me that the CD is not big enough,
   even when using 700 MB CD-Rs. When I look on the harddisk I see that
   the files are more than 800 MB in size. Why?
 A:700 MB is the storage space for data CDs. Data has a third layer of
   error correction which need more storage space. So sector size is 2048
   bytes for data and 2352 bytes for audio. There are around 360000
   sectors on a 700 MB CD-R, that is 737280000 bytes = 703 MB for data
   sectors. On audio CDs this is 846720000 bytes = 807 MB. This is why the
   files are too big to write them as data files, but it should be
   possible to write them as audio CD instead.


 Q:I get a message stating that it could not detect my CD-ROM read
   settings or that it can't find a matching read mode. What can I do?
 A:Sometimes EAC will autodetect a wrong read command. Try to manually
   select a read command. In the Drive Options, go to Read Commands page
   and select the Read Command MMC1 manually (or any other that works).
   Test it with burst mode. If you tested all of them, but none of them
   worked, try to extract with another program like WinDAC or CDEx. If
   both also fails, make sure that your drive is capable of extracting
   digital audio at all.


 Q:When I extract, the extraction proceed very fast, but when I listen to
   the resulting files, they are all silent. What did I do wrong?
 A:Sometimes EAC will autodetect a wrong read command. In this case it is
   possible that only silence is returned. Try to manually select a read
   command. In the Drive Options, go to Read Commands page and select the
   Read Command MMC1 manually (or any other that works). Test it with
   burst mode. If you tested all of them, but none of them worked, try to
   extract with another program like WinDAC or CDEx. If both also fails,
   make sure that your drive is capable of extracting digital audio at
   all.


 Q:When I try to start EAC or to compress/decompress, I immedately get 
   an Access Violation. Why does this happen?
 A:Usually this error occurs when not using the ASPI interface of Adaptec.
   So try at first to install it on your computer. When you use Windows
   NT/2000, the native SCSI interface could also make some problems, so
   also install the Adaptec interface in that case.
   Second, it has also happened that an illegal audio codec let EAC crash
   on enumerating all audio codecs. In that case try to disable (not
   deinstall) each codec and try again, you could enable the codecs then
   again piece for piece to find out which one causes the problem. Mainly
   some versions of LAME and OggVorbis ACM codecs cause this behaviour
   (included in e.g. Nimo Codec Pack).


 Q:Since I installed a new CD-ROM drive, EAC does not work at all or not
   correct anymore. What can I do to make it work again?
 A:In this case it is always a good idea to delete the EAC entry in the
   registry. So start regedit.exe and delete the key at
   HKEY_CURRENT_USER\Software\AWSoftware\EAC


 Q:What is "Paranoid Mode" and why is it not recommended?
 A:This mode is the oldest read mode in EAC, it exists from version 0.1b
   on. It will read every sector twice, but in very small blocks. This
   will slow down extraction, no drive features are used. If the drive
   does caching the option below should be activated, but this could
   create problems on some drives. This mode is stressing the drive very
   much and should not be used, if one of the other secure modes works ok.
   The "disable CD-ROM drive cache" will disable the drive cache when
   using Paranoid mode, by resetting the drive after a read command. On
   some drives this will take several seconds and should not be used in
   that case.


 Q:Why should I use Test & Copy? How to read the CRC codes?
 A:If you don't like to use the secure modes, and the burst mode does not
   have error correction, the best possibility to check if an error
   occured is to copy and test the track. For each read and each track,
   the appropriate CRC column is filled with the actual CRC code. One CRC
   code is unique for a set of data. So by comparing the CRC values you
   could be quite sure that both reads resulted in the same file.


 Q:What is C2?
 A:On all CD-ROM media are at least two levels of error correction, called
   C1 and C2. If both fail, the output is probably not correct anymore.
   Most drives are not able to report if audio reads failed or not, so
   each block had to be read twice and be compared to make sure that
   everything is fine. But some newer drives are able to report if C1/C2
   failed on specific samples on a read, making it possible to read only
   once and see if a read error occured. But there is still a problem, as
   some drives do not report these errors correctly, so you should test it
   thoroughly before trusting the results.


 Q:Then how does it come that a CD that plays on my standalone CD player
   without any pop or any other error, makes that difficulties on
   extraction?
 A:Standalone CD players perform oversampling and some more error
   correction. Further, if the error is too big to be corrected, it will
   perform "error hiding". That means that the player will hide the error
   in a way that it is not audible to the common listener. These
   additional techniques are not implemented in the CD-ROM drives, thus
   the uncorrected data is given back.


 Q:I had ripped other records, they extracted fine. But there was one CD,
   where the ripping was desperately slow and the peak level of what I got
   was always 0%. Sometimes I got "Sync Errors". I tried several times
   without success. What can I do then?
 A:Have a look on the CD if it is dirty. Try to clean it (from the inner
   ring to the outer bound), perhaps it works better then. If not, try to
   lower speed or even to extract in burst mode, sometimes this will give
   better results (but no error reporting though).



 Q:When using burst mode, EAC also shows up timing problems, are these
   really errors or what?
 A:No, burst mode has no error detection nor error correction. If burst
   mode brings up a timing problem, the read command needed a lot of time,
   which could have several reasons, like loosing sync or trying to fix an
   read error. Of course this is a really poor "error detection" and
   should not be taken as serious indication.


 Q:I didn't configure EAC at the first time and EAC extracted the audio
   really fast, somewhere between 8x and 14x. This seems too fast for an
   exact extraction?
 A:In default configuration EAC uses the burst mode. I recommend to use
   the appropriate secure mode for your drive. To know what the
   appropriate read mode is, there is an automatic feature test in the
   drive options, just below the read mode switches.


 Q:I only get many pops and clicks when extracting a very badly scratched
   CD in secure mode, what can I do?
 A:It could possible to revive them by copying them in burst mode to hard
   disk. The high readout speed keeps the optical system of the drive from
   following the scratches instead of the audio track. After copying check
   the copies out, perhaps there were still errors left.



 Q:I sometimes get a sync error when I extract a track. The thing is it's
   not always with the same disc that I'm burning from BUT it is always in
   the same spot. Is there an explanation for this?
 A:Some Toshiba drives have a firmware bug returning wrong data on special
   positions of every CD. As the error really occured, you should listen
   to these suspicious position allways and decide if the error is audible
   or not.


 Q:What does the Track Quality really mean? A few times I get 99.7% or
   97.5%. But there are no suspicious position reported.
 A:When you get 99.7% and so on, that means that a bad sector was found,
   but the secure mode has corrected it - from 16 times of grabbing the
   sector, there were 8 or more identical results. So it only indicates
   read problems. It is the ratio between the number of minimum reads
   needed to perform the extraction and the number of reads that were
   actually performed. 100% will only occur when the CD was extracted
   without any rereads on errors. ONLY when there are suspicious positions
   reported, there are really uncorrectable read errors in the resulting
   audio file.


 Q:I often get files with a Peak Level below 90%. What is this Peak Level
   for?
 A:The Peak Level of a song the maximum volume within the song. So 100%
   will have the maximum volume possible in a file. A file with Peak Level
   50% will have only at its loudest point half of the maximum possible
   volume. So this is no quality information, it is useful for creating a
   CD mixed of tracks from different CDs and for normalizing.


 Q:I would like to let EAC automatically create directories named from
   artist or album name. Is this possible somehow?
 A:You can set this in the filename option. If you use the '\' character,
   EAC will create all these subdirectories. For example %a\%n - %t
   But you may not specify an absolute path like c:\%a\%n nor \%a\%t
   For more information read the tooltip of this option.


 Q:EAC grabs only at speed 4x in secure mode, surely. Is it normal?
 A:That is because in secure mode EAC reads every sector at least twice.
   This is normal. Try setting the speed to maximum, for some Teac drives
   a firmware update will improve speed settings.


 Q:On extraction EAC reports "Can't Open Selected Codec". Why?
 A:Go To Compression Options, and check if all compression options are
   correct. If you don't want to compress your files, make sure that there
   is "Internal Wav Routines" selected.


 Q:When doing my very first CD rip, I got quite different size files. EAC
   produced a 867 KB Wav file, while Cdex produced a 21,806 KB Wav file on
   my hard drive. These two Wav files both played back fine using Winamp.
   So I have no idea as to why the two file sizes are so different?
 A:If both files played the complete track, it looks like you produced a
   compressed WAV with EAC. In EAC, enter F11 and make sure the Waveform
   tab shows "Internal WAV routines" for Wave format. This will produce a
   WAV file that is about 176kB for every second of music.


 Q:When I extract tracks with EAC and write them to a CD-R with a burn
   program, I get 2 second gaps between each track. Why does EAC insert
   them?
 A:EAC does not insert the gaps. These gaps are inserted by the writing
   program. There are two possibilities how these gaps could occur. Once
   if you write in TAO (Track At Once), there have to be a gap between
   tracks, so use DAO (Disc At Once) instead. Second, if you already use
   DAO, you should examine that program options, somewhere will be a flag
   where the standard 2 second gap could be deactivated.


 Q:If EAC encounters problems with an extraction, it slows down, which is
   fine. The problem is, it continues to read slowly on subsequent tracks,
   even if those tracks would not otherwise cause problems. I have
   verified this by stopping the process and restarting on another track
   that was extracting slowly; after restarting, it extracts full speed
   with no problems. What can I do?
 A:If you have selected "Allow Speed Reduction" and the speed box also
   shows different possible speeds, then the problem lies within the
   reader. It could help to use the cool down feature (let it cool down
   every 15-30 min for several minutes, perhaps this already solves it).
   Otherwise don't use the flag "Allow Speed Reduction", but of course
   then it won't read anymore that accurate on bad sectors.


 Q:I have clicked on the "Possible Errors" after extraction, and then I
   have to "Select A Track". I do that and then I have 2 choices: Glitch
   Removal and Play. If I do any of these both, the whole track will be
   processed, I'm not sure where to find the position of the flaws.
 A:When finished extracting, EAC will tell you if there were errors in the
   extraction. If there were, when you click the "Possible Errors" button,
   it will give you a time range that the error occured in. If it doesn't
   report errors, it will not have a range, you will be able only to
   choose the whole track and not the specific positions (as there are
   none).


 Q:If I have some glitches in a WAV after extraction, and I didn't hit the
   glitch removal button before I got out of that menu, is there a way to
   access glitch removal after this point?
 A:On the top select Tools, then Process WAV. Select song from wherever
   it's saved. Anything can be done to this file or any uncompressed WAV
   file. When you want to removing glitches, you have to select that
   faulty range of the WAV for doing glitch removal (of course, you are
   able to select the whole waveform by double clicking it).


 Q:I burned a continous CD in TAO by accident... Is it possible to remove
   the standard 2 second gap automatically?
 A:Best possibility would be to extract all tracks with a read offset of
   -5000 and then load each track into the EAC WAV editor and use "Remove
   leading and trailing silence". Then you should be able again to write
   them without gaps. It would be possible to remove them also by offset
   correction and gap detection, but for that you would need and use the
   exact combined offset of the writer.


 Q:I read that it is possible to leave out the pre-gap of a track.
   Unfortunately, I could not find where these options could be set.
 A:In the Action menu, you could choose what to do with the gaps. For a
   new extraction, try to detect gaps, then choose "Leave Out Gaps" and
   copy the tracks. Usually the gaps are not copied to the (single) WAV
   files anymore.


 Q:What is the difference between Gap Detection Methods A, B, & C ?
 A:These are all different methods for retrieving the index markers (gaps,
   etc.). Some methods will work with some drives, the others won't, you
   should test all of them which works best for you. None of them is by
   used method better or worse than the other, but by used method the A is
   the fastest one and C the slowest (if it works correctly!).


 Q:Should I be selecting Accurate, Inaccurate, or Secure in the "Gap
   Detection Accuracy" box?
 A:Accurate Accuracy should be quite good for any CD. If there is a
   problem CD, where the gap detection hangs, try inaccurate, as it will
   go on, when no information could be gathered in a time. If you got gap
   length that are wrong only by some blocks, you could try to do gap
   detection again with secure settings.


 Q:When using "Copy Image And Create CUE sheet" (or just creating a CUE
   sheet), EAC says it is getting pre-gap info on Track 1, the CD is
   spinning furiously, but nothing is getting written to the HD. I've left
   it as long as 2 hours, nothing changes in the GUI, no progress bar, no
   file gets created, nothing. (But I can cancel the operation.) What's
   up?
 A:Try to select another "Gap Detection Mode" in the drive options. If the
   selected mode does not work like that one, one of the other two should
   work at least.


 Q:The last few audio CD's I've copied using EAC all have the track
   position wrong by about 1 second. If I go to a particular track with my
   CD player, it will start the track about 1 second INTO the audio track.
   I have been using the "Copy Image And Create CUE Sheet" option for
   copying the CD's. How can I avoid this problem in the future?
 A:One of the biggest mistakes that could be made in 0.85beta (from
   0.9beta3 on I prevented it automatically) is to have selected "Remove
   Leading And Trailing Silence". If the image file contains silence at
   the beginning (e.g. 1 second) it will be removed and everything get
   moved by one second. So you should deactivate this option for 0.85b4.
   If this is not the problem, try a different gap detection mode and
   compare the generated CUE sheets manually.


 Q:When using a CUE sheet generated by EAC in CDRWin, it tells, that the
   CUE sheet is not valid. When I have a look at the CUE sheet myself, I
   see that there are sometimes dozens of indecies that all have the same
   position. What can I do?
 A:Try a different gap detection mode and if none removed that problem,
   you would have to edit these CUE sheets manually, removing all indecies
   bigger then 01 and indecies that have impossible possitions.


 Q:Ripping cd is saved as *.cgf and I don't know why. I have used eac
   before and it worked perfect. Now it stuck saving as *.cgf.
 A:Go to compression options and have a look if you selected "Do not write
   WAV header" and specified "cgf" below.


 Q:I am getting Sync and Read errors occasionally, but EAC will still
   finish ripping, though with some "suspicious" positions. What to do
   now?
 A:Clean the CD carefully and try again. If the errors don't go away,
   listen to the suspicious positions and decide whether they are audible
   or not. You could also try to rip these tracks in burst mode, sometimes
   the reader could get better results on these bad sectors.


 Q:If I rip a track in secure mode (Hitachi GD 2500, accurate stream, no
   cache, c2 correction) and during the rip process the correction
   indicator gets higlighted and then continues ripping. The EAC report
   indicates "No error" but when I hear the resulting wav file there is an
   error in it (a blank at the position where the correction indicator got
   highlighted)! The rest of the track is perfect of course. There is only
   this small blank.
 A:It seems that C2 is not correctly implemented in some drives. To be on
   the safe side, you should turn off the C2 error correction.


 Q:I have TEAC 532E-B and EAC says that the drive is capable of retreaving
   C2 error information. But EAC doesn't report all errors in that mode!
 A:It seems that C2 is not correctly implemented in some drives. To be on
   the safe side, you should turn off the C2 error correction.


 Q:I have an Afreey drive and during extraction EAC sometimes hangs. What
   can I do?
 A:It is still not known what causes this problem, there are Afreey users
   without any problems and some others have this problem. It is possible
   to continue the extraction by pressing the eject button on the drive.
   Try to play around a little bit with your options (DMA or deinstall
   busmaster drivers), probably it won't help, but perhaps it does.


3. Compression Questions

 Q:I want to compress audio tracks to MP3s, what do I need besides from
   EAC?
 A:Remember that EAC does not supply a MP3 codec; you may use the LAME,
   Gogo or the BladeEnc DLL's (or FAAC Dll for AAC compression) by copying
   them into the same directory where you copied EAC. Then you will be
   able to choose the installed DLLs in the compression option dialog box.
   Of course the quality of MP3 is based on the encoder and the bitrate
   you use. Beside the DLLs you could also specify external command line
   compressors that will be executed after an entire track was read (and
   not on-the-fly).


 Q:I'm trying to decode mp3 to wav's but it keeps telling it can't find
   codec. I know about the encoding dll issue, but this one has me
   stumped.
 A:For decompression of MP3s the Fraunhofer MP3 Codec needed to be
   installed. It is sufficient to use the "advanced" Codec (not the
   "professional"). The advanced codec is part of windows. On older
   windows it could be installed by updating the media player... (Should
   be updated with the other codecs). The installed codec should then be
   listed in EACs codec list.


 Q:What is a compressed Wav file and how does it differ in quality from a
   regular wav file or from a MP3 file?
 A:There are two groups of audio data, compressed and uncompressed data.
   The compressed group could also be splitted to lossless and lossy
   compression. Lossless compression is like having uncompressed data,
   only that the file is only around 70% of the uncompressed size
   (Comparable to compression with WinZIP). To the group of lossy
   compression also belongs MP3, it is not possible to recreate the
   original audio file 100%, there are frequencies missing, etc. Now, MP3
   is ONE lossy compression format, there are others like AAC, MP2, TAC,
   etc. The nice side on WAVs is that it could be wrapped on any
   compression for which an audio codec exists in Windows. So if you own
   the Fraunhofer Codec (or the LAME/Blade/Gogo DLL) you could produce
   MP3-WAVs. These are standard MP3 files, but having a small header
   preceeding the actual data telling the player what codec to use for
   playing/decompression. So these files could be played with any media
   player or any other sound tool. As the header does not matter on MP3
   compression, you could even rename the MP3-WAVs from .wav to .mp3
   without loosing playability by a MP3 player.


 Q:What is VBR?
 A:It is short for "Variable Bitrate". Some MP3 encoder support this. When
   enabled the compressor will use a bitrate that would fit the actual
   passage. If it is a very complex part it will use a quite high bitrate
   and e.g. on silence or easy parts it will use a lower bitrate. So
   usually the average bitrate will be not as high as a MP3 of same
   quality with constant bitrate.


 Q:I use the Fraunhofer Codec or an encoder DLL to compress to MP3, but
   the resulting File has the file extension ".wav". What is wrong?
 A:EAC will write WAVs when using codecs (EAC emulates a codec for the MP3
   DLLs). This has the advantage that it will play with any media player,
   when any version of the Fraunhofer codec is installed (even the free
   one, called "advanced"). If you want "pure" MP3 files (without the WAV
   header in front of it), just select the option "Do not write WAV
   header" and specify the appropriate file extension below (".mp3").


 Q:I tried to compress with the Fraunhofer MP3 codec, but I am only able
   to compress audio with only very low bitrates. How am I able to
   compress with higher bitrates?
 A:Make sure that you do not use the Fraunhofer advanced codec, as that is
   the free version, that will only allow specific compression rates. To
   compress with higher bitrates, use the professional version of the
   codec, or use any of the supported encoder DLL or any of the supported
   external command line encoders.


 Q:Why can't I use WMA at 160 kbits?
 A:Microsoft only allows encoding with 160 and more if a copy protection
   scheme is activated. This makes some more work, and I don't like to add
   copy protection to directly ripped songs. I heard that Microsoft
   already put aside that policy, so perhaps it will be possible in future
   versions.


 Q:I am using an IBM laptop, and the BladeEnc.dll, EAC says that I got a
   100% rip, but when I play the file, it sounds like the singer is under
   water.
 A:Blade is poor at bit rates below 160, maybe 192. So user higher
   bitrates, or use a different encoder that works better with lower
   bitrates like Fraunhofer or LAME.


 Q:Which flags can I use in the external compression scheme "User Defined
   MP3 Encoder"?
 A:In the field "Additional command line options" you could use
   replacements for the selectable options :

    %s        Source filename
    %d        Destination filename
    %h...%h   Text "..." only when "High quality" selected
    %l...%l   Text "..." only when "Low quality" selected
    %c...%c   Text "..." only when "CRC checksum" selected
    %r        Bitrate ("32".."320")
    %a        CD artist
    %g        CD title
    %t        Track title
    %y        Year
    %n        Track number
    %m        MP3 music genre
    %o        Original filename (without temporary renaming)
    %e        Comment (as selected in EAC)

   So a command line would look like (for l3enc)
     %s %d -br %r000 %h-hq%h %c-crc%c
   The extension can also be selected for this setting.


4. Offset Questions

 Q:Is the read offset (or the write) offset drive model dependent, or is
   it possible that the same drive has a different offset in a different
   system?
 A:The offsets should be the same for all drives of that specific model.
   Though, it is possible (but not probable) that the offset varies with
   different firmwares.


 Q:What is the difference between read offset, write offset and the
   combined read/write offset?
 A:Read offsets occur on reading (extracting). Write offsets happen on
   writing (burning) a CD-R. Most CD record programs do not support write
   offsets (as EAC perhaps do not support your writer for burning). So, to
   create an exact (offset corrected) copy of your CD, you would have to
   compensate the write offset already on reading. So instead of specifing
   the read offset as sample offset for extraction, you would rather use
   the combined read/write offset. This is easily calculated by the
   formula: Read Offset + Write Offset = Combined Read/Write Offset


 Q:What is an read or write offset? When do they occur?
 A:During extraction or writing of the audio data, nearly all CD-ROM/CD-R
   drives will add an offset to the position. This is usually around
   500-700 audio samples (ca. 1/75 second) on reading and around 0-18
   samples on writing (ca. 1/1000 second). So if a program queries a
   specific sector, it will not receive exactly that sector, but shifted
   with the number of samples of the offset.


 Q:How do you find your CD-ROM's read offset?
 A:There is a test routine included in EAC that will determine the offset
   for a drive using a library of predefined commercial CDs. It is
   important that you use exactly the same pressing as the creator,
   otherwise another offset could be occured on remastering. So you should
   at least receive twice the same offset on two individual CDs. If you
   have a Plextor 40X CD-ROM drive (or know somebody who owns one), you
   could even help to extend that database of included offset CDs to help
   others to determine the offsets. If this does not bring a good result,
   the last option is to ask the other persons in the mailing list if
   anybody already determined the offset for the specific CD-ROM drive
   model.


 Q:How do I determine the combined read/write offset?
 A:The combined read/write offset is only valid for the special
   combination of exactly one reading drive and exactly one writing drive.
   If you use another reading, you would most probably need a different
   combined offset. To determine this offset, you would need to write a
   CD-R/CD-RW. At first prepare WAV files you want to write to the CD.
   Then write it to a CD (either with any burning program, or with EAC
   using write offset 0). Do not delete the written WAV files. Afterwards
   you have to extract one or more tracks from the freshly burned CD,
   using the specific reader and using read offset 0. Of course you should
   not overwrite the original WAV files. Now you have to use the WAV
   Compare feature in EAC to compare the first WAV (original) with the
   second (reextracted one). Usually EAC will report either missing
   samples or extreneous samples. The number that is reported by that will
   be your combined offset, only be changed to positive or negative. If
   your original file has extreneous (repeated) samples or the copied file
   has missing samples the offset should be positive, otherwise it should
   be negative. (I hope this is correct) To double check the found offset,
   use that offset as sample offset for reading. Now The reextracted file
   and the original should be the same without missing or extreneous
   samples.


 Q:How do I determine the CD-Rs write offset?
 A:At first determine your read offset, then determine the combined
   read/write offset. By using this formula, you will get the write
   offset. Write Offset = Combined Read/Write Offset - Read Offset


 Q:I try to determine the offset for my CD reader using a CD from the list
   given on EACs homepage, but it tells "CD not found in offset database".
   Why?
 A:It has to be the same pressing like I used, as different pressings
   usually uses a different offset. This specific error occurs, when the
   track layout is different than the correct CD, e.g. one track is
   slightly longer (1 sector would be enough).


 Q:I used several CDs to determine the sample offset for my CD reader, but
   the results of the offsets are not consistant (all the same). What now?
 A:Probably you use different pressings of some (or all of) the CDs you
   tested. If you get at least twice exactly the same offset, you could be
   pretty sure to have found the correct one (and only then!).


5. Write Questions

 Q:I have experienced the following problem after making some audio-cd
   copies : several tracks on the disk cannot be accessed directly on my
   audio cd-player although when the cd is played continuously it works
   fine. If I am using for playing the cd my cd-rom or my writer
   everything is OK and I can directly access all the tracks.
 A:This happen sometimes, when the writer starts loosing the ability to
   find the correct positions for writing and the actual gaps are not 100%
   on the correct positions. Usually this happens to Yamaha writers sooner
   or later. So try to lower the writing speed and try different CD-R
   media. But it is also possible that a writer is not able to write very
   short gaps, so make sure that in the CUE sheet each gap is bigger than
   at least 100 sectors (1 1/3 second).


 Q:I was wondering if I could copy a CD on the fly with EAC. I could not
   find any menu or option for that function. It would be useful if it
   worked because I could have offset corrected copies without having to
   copy the files/image first on the hard disk. Will it be supported in
   the future?
 A:"On-the-fly" copies will never be supported in EAC. This tool is used
   for secure copies, and secure copies can't be burned "on-the-fly" (OK,
   with the new burnproof feature it would be possible, but not
   recommended anyway).


 Q:I want to make copies of my CDs and add CD-TEXT because my car cd
   player can read that. How do I do it?
 A:It is done with the cue sheet, you (or EAC) can add TITLE and PERFORMER
   tags (enable it in EAC options). If you want to burn with EAC, you will
   also find some CD-Text options in EAC options and don't forget to
   activate it in the Drive options. In the Layout Editor, you could also
   still change title and artists.


 Q:I have an audio CD which includes a CD-Extra segment. There are 11
   audio tracks, the extra track 12 is indicated in EAC by a "file icon"
   instead of "music icon". I can't seem to determine how to produce a cue
   sheet which will allow the CD-Extra to be written via CDRWin. What is
   the recommended procedure for extracting the cue sheet from an audio CD
   which includes a CD-Extra segment?
 A:As the data track has to be written in a second session(!) it is not
   possible to reproduce the complete CD with ONE cuesheet. Therefore you
   should burn at first the audio tracks, close the session (and leave the
   disk open). Then you could write the data track. I suggest writing the
   data files individually instead of writing an data image.


 Q:When trying to write a CD using EAC, I get a Write Error - Send CUE
   Sheet or Write Parameter Page error, what does that mean?
 A:EAC does not support all writers yet. At the moment only MMC writer
   that are able to write CDs using CUE sheets (not in RAW mode). So if a
   write error occur, the drive is most probably not supported.


 Q:When I begin writing, EAC stops suddenly with an error, sometimes with
   no additional informations, what can I do?
 A:EAC does not support all writers yet, so it is possible that EAC just
   do not work correctly with that drive. Further it would be possible
   that something in your system will break the stream to the writer,
   resulting in a buffer underrun. Make sure that there are no other
   applications are running while writing.
   If could try to switch the sync data transfer on for the writer, you
   could find that option in the Windows Device Manager (System
   Properties), there select the writer and show up and edit the
   properties of that drive.


6. WAV Editor Questions

 Q:What is Normalization?
 A:Normalization is used to bring up the sound level on songs that were
   not recorded very loud. It is use full when making a compilation disc
   as the songs that you use may have been recorded at all different
   levels. But be aware that on some discs the volume was choosen to
   create a special effect, on these CDs normalization would destroy that
   effect.


 Q:What is DC Offset?
 A:DC offset occurs when the average/mean of the signal is a value other
   than 0 which means on average DC current flows through a circuit and
   which means the signal will clip earlier on one side (top or bottom)
   and your maximum signal strength before clipping occurs is smaller. To
   get rid of DC offset the average of the signal is subtracted form every
   sample of the signal.


 Q:I have recorded and saved a noise wav (named nrp). I appear able to
   open it but am unable to subtract the noise profile from my subject wav
   (the "Reduce Noise" option is inoperable.) Any ideas om what I am doing
   wrong?
 A:After created the noise profile (selecting a range, create noise
   profile, save noise profile) you are able to load the wav to denoise
   (or keep the actual one). There you have to load a noise profile first
   (noise profile/load), or keep the noise profile you created from that
   audio file, then you are able to remove the noise of it. You have to
   select first a range of the audio data that should be denoised before
   the menu option will be activated.


 Q:Can you use EAC to take pops/clicks out?
 A:I assume that you are recording the CD to WAV and then using the WAV to
   burn a rw-cd. There's an extra step in the middle to edit the clicks
   out of the WAV file. More complex pops that occur on analog recording
   (tapes, etc.) should be found by listening to the WAV roughly to find
   the positions with +/- 3 seconds accuracy. Then select such a range and
   choose "Pop Detection". Usually EAC will find them automatically. If
   not, switch to "Spectral View" and look for any anormalities. Then you
   have different options to remove the pop.


7. Utilities Questions

 Q:How to perform CDDB queries in batch mode?
 A:Just insert all CDs you want to query into the actual drive EAC uses
   (do not edit any data!), afterwards press Alt-P.


 Q:What are "Alternate CD Play Routines"?
 A:These routines will playback audio tracks by extracting the data and
   directly playing them through the soundcard. It is not necessary that
   the drive is connected to the soundcard by a cable.


 Q:I tried to select several files at once, but afterwards, the first and
   last file changed place. What can I do?
 A:In windows kernel is a bug, that occurs when selecting multiple files
   at once (e.g. in write dialog or in ID3Tag dialog). The first and last
   file name will be exchanged. This could result in some problems, so
   with the option "Correct bug of wrong filename order in Windows
   multiple file dialog" EAC will again exchange the first and last
   filename to the correct order.
